//Generated ALM file 000057_00d9_02.alm
//Byte, 0, Bit, Alarm Desc, Category
1	0	8	Alarm State	General
1	0	7	Warning State	General
1	0	6	Emergency Trip Active	General
1	0	5	Calibration Recommended	General
1	0	4	Limit Switch Closed Activated	General
1	0	3	Limit Switch Open Activated	General
1	0	2	Calibration Running	General
1	0	1	Device Write Protected	General
2	0	8	Test Initializing	General
2	0	7	Test Running	General
2	0	6	Automated PST Active	General
2	0	5	Manual PST Active	General
2	0	4	Pneumatic Test Active	General
2	0	3	Emergency Trip Test Active	General
2	0	2	Free	General
2	0	1	Testing Not Allowed	General
3	0	8	Unintended Valve Movement	General
3	0	7	Valve Open Stuck	General
3	0	6	Valve Close Stuck	General
3	0	5	Valve Intermediate Stuck	General
3	0	4	Supply Pressure Out of Limits	General
3	0	3	Supply Pressure Drop	General
3	0	2	Too Large Housing Pressure	General
3	0	1	Temperature Out of Limits	General
4	0	8	Spool Valve Stuck	General
4	0	7	Pneumatics Problem	General
4	0	6	PST Pressure Drop	General
4	0	5	PST Overshoot	General
4	0	4	Valve Opening Time High Limit Exceeded	General
4	0	3	Valve Closing Time High Limit Exceeded	General
4	0	2	Loop Current Below Low Limit	General
4	0	1	Free	General
5	0	8	Valve Full Strokes Limit Exceeded	General
5	0	7	Actuator Full Strokes Limit Exceeded	General
5	0	6	PST Counter Limit Exceeded	General
5	0	5	Total Operation Time Limit Exceeded	General
5	0	4	Free	General
5	0	3	Free	General
5	0	2	Free	General
5	0	1	Free	General
6	0	8	Temperature Trend Low Limit	General
6	0	7	Temperature Trend High Limit	General
6	0	6	Supply Pressure Trend Low Limit	General
6	0	5	Supply Pressure Trend High Limit	General
6	0	4	PST Breakaway Pressure Low Limit	General
6	0	3	PST Breakaway Pressure High Limit	General
6	0	2	PST Load Factor Low Limit	General
6	0	1	PST Load Factor High Limit	General
7	0	3	Critical Power Failure	General
7	0	2	Device variable alert	General
7	0	1	Maintenance required	General
11	0	4	Quinary Analog Channel Saturated	General
11	0	3	Quaternary Analog Channel Saturated	General
11	0	2	Tertiary Analog Channel Saturated	General
11	0	1	Secondary Analog Channel Saturated	General
14	0	4	Quinary Analog Channel Fixed	General
14	0	3	Quaternary Analog Channel Fixed	General
14	0	2	Tertiary Analog Channel Fixed	General
14	0	1	Secondary Analog Channel Fixed	General
15	0	8	Pressure Sensor 1 Failure	General
15	0	7	Pressure Sensor 2 Failure	General
15	0	6	Supply Pressure Sensor Failure	General
15	0	5	Temperature Sensor Failure	General
15	0	4	Position Sensor Out of Range	General
15	0	3	Position Sensor Failure	General
15	0	2	Input Signal Sensor failure	General
15	0	1	Free	General
16	0	8	PST Failed	General
16	0	7	Emergency Trip Test Failed	General
16	0	6	Pneumatics Test Failed	General
16	0	5	Safety Electronics Test Failed	General
16	0	4	Ready to Reset	General
16	0	3	Safety Position Requested	General
16	0	2	LCP Communication Failure	General
16	0	1	Free	General
27	0	8	Field device malfunction	Overview
27	0	7	Configuration change	Overview
27	0	6	Cold start	Overview
27	0	5	More status available	Overview
27	0	4	Primary variable analog output fixed	Overview
27	0	3	Primary variable analog output saturated	Overview
27	0	2	Non-primary variable out of limits	Overview
27	0	1	Primary variable out of limits	Overview
28	0	2	Device Mfg/Type/Rev Mismatch	DeltaV
28	0	1	Analog/Digital Disparity Detected	DeltaV
30	0	8	Proof Test Overdue	DeltaV
30	0	7	Proof Test Due Soon	DeltaV
30	0	3	External Advise Condition	DeltaV
30	0	2	External Maint Condition	DeltaV
30	0	1	External Failed Condition	DeltaV
