DEVICE_MANUFACTURER NAME="Neles Automation."
{
     HART_MANUFACTURER_ID=87
}
HART_DEVICE_TYPE NAME="VG9000H" DEVICE_TYPE_ID=217 MANUFACTURER="Neles Automation." 
{
     DESCRIPTION="Neles Automation. VG9000H"
}
HART_DEVICE_REVISION REVISION="2" DEVICE_REVISION_ID=2 MANUFACTURER="Neles Automation." HART_DEVICE_TYPE="VG9000H" 
{
     DESCRIPTION="Neles Automation. VG9000H Rev 2"
     DDREV=201
     RESOURCE_PATH="000057\00d9\"
     FACEPLATE_DISPLAY_NAME=""
     ALARMS_ENABLED=T
     DEVICE_ALARM NAME="MAINT_ALM"
     {
        ENABLED=T
        PRIORITY_DEFAULT=ADVISORY_1
        PRIORITY_OBJECT_INDEX=0
        ALARM_OBJECT_INDEX=0
     }
     DEVICE_ALARM NAME="FAILED_ALM"
     {
        ENABLED=T
        PRIORITY_DEFAULT=WARNING_1
        PRIORITY_OBJECT_INDEX=0
        ALARM_OBJECT_INDEX=0
     }
     DEVICE_ALARM NAME="COMM_ALM"
     {
        ENABLED=T
        PRIORITY_DEFAULT=WARNING_1
        PRIORITY_OBJECT_INDEX=0
        ALARM_OBJECT_INDEX=0
     }
     DEVICE_ALARM NAME="ADVISE_ALM"
     {
        ENABLED=T
        PRIORITY_DEFAULT=ADVISORY_1
        PRIORITY_OBJECT_INDEX=0
        ALARM_OBJECT_INDEX=0
     }
     ATTRIBUTE_INSTANCE NAME="DEV_PT_REMINDER"
     {
        VALUE { CV=0 }
     }
     ATTRIBUTE_INSTANCE NAME="DEV_PT_TIME"
     {
        VALUE { CV=0 }
     }
     ALARM_MASK TYPE=FAILED_MASKS
     {
        MASK48= { 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 }
        MASKSUBSYS= {00 00 01 00}
        MASKSTATS= {00 80}
     }
     ALARM_MASK TYPE=MAINTENANCE_MASKS
     {
        MASK48= { 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 }
        MASKSUBSYS= {03 00 82 00}
        MASKSTATS= {00 07}
     }
     ALARM_MASK TYPE=ADVISORY_MASKS
     {
        MASK48= { ff ff ff ff ff ff 07 00 00 00 0f 00 00 0f ff ff 00 00 00 00 00 00 00 00 00 }
        MASKSUBSYS= {00 00 44 00}
        MASKSTATS= {00 68}
     }
     ALARM_MASK TYPE=SUPRESS_MASKS
     {
        MASK48= { 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 }
        MASKSUBSYS= { 00 00 00 00 }
        MASKSTATS= { 00 00 }
     }
}
