<?xml version="1.0" encoding="utf-8"?>
<AlertsRoot Version="1.0">
  <Protocol>HART</Protocol>
  <Manufacturer>87</Manufacturer>
  <DeviceType>217</DeviceType>
  <DeviceRevision>2</DeviceRevision>
  <DDRevision>2</DDRevision>
  <VariableList>
    <Variable>
      <Size>1</Size>
      <Type>bit-enumerated</Type>
      <BytePosition>0</BytePosition>
      <Label>
      </Label>
      <Name>TODO_Find_Name</Name>
      <AlertList>
        <Alert>
          <Value>256</Value>
          <AlarmString>Device Not Responding</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
      </AlertList>
    </Variable>
    <Variable>
      <Size>1</Size>
      <Type>bit-enumerated</Type>
      <BytePosition>0</BytePosition>
      <Label>Device status</Label>
      <Name>device_status</Name>
      <AlertList>
        <Alert>
          <Value>1</Value>
          <AlarmString>Primary variable out of limits</AlarmString>
          <Severity>ALERT_MAINT_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>2</Value>
          <AlarmString>Non-primary variable out of limits</AlarmString>
          <Severity>ALERT_MAINT_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>4</Value>
          <AlarmString>PV Analog Channel Saturated</AlarmString>
          <Severity>ALERT_MAINT_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>8</Value>
          <AlarmString>PV Analog Channel Fixed</AlarmString>
          <Severity>ALERT_ADVISE_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>16</Value>
          <AlarmString>More status available</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>32</Value>
          <AlarmString>Cold start</AlarmString>
          <Severity>ALERT_ADVISE_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>64</Value>
          <AlarmString>Configuration changed</AlarmString>
          <Severity>ALERT_ADVISE_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>128</Value>
          <AlarmString>Field device malfunction</AlarmString>
          <Severity>ALERT_FAILED_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
      </AlertList>
    </Variable>
    <Variable>
      <Size>1</Size>
      <Type>bit-enumerated</Type>
      <BytePosition>1</BytePosition>
      <Label>Status group 0</Label>
      <Name>device_specific_status_0</Name>
      <AlertList>
        <Alert>
          <Value>128</Value>
          <AlarmString>Alarm State</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>64</Value>
          <AlarmString>Warning State</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>32</Value>
          <AlarmString>Emergency Trip Active</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>16</Value>
          <AlarmString>Calibration Recommended</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>8</Value>
          <AlarmString>Limit Switch Closed Activated</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>4</Value>
          <AlarmString>Limit Switch Open Activated</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>2</Value>
          <AlarmString>Calibration Running</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>1</Value>
          <AlarmString>Device Write Protected</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
      </AlertList>
    </Variable>
    <Variable>
      <Size>1</Size>
      <Type>bit-enumerated</Type>
      <BytePosition>2</BytePosition>
      <Label>Status group 1</Label>
      <Name>device_specific_status_1</Name>
      <AlertList>
        <Alert>
          <Value>128</Value>
          <AlarmString>Test Initializing</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>64</Value>
          <AlarmString>Test Running</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>32</Value>
          <AlarmString>Automated PST Active</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>16</Value>
          <AlarmString>Manual PST Active</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>8</Value>
          <AlarmString>Pneumatic Test Active</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>4</Value>
          <AlarmString>Emergency Trip Test Active</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>2</Value>
          <AlarmString>Free</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>1</Value>
          <AlarmString>Testing Not Allowed</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
      </AlertList>
    </Variable>
    <Variable>
      <Size>1</Size>
      <Type>bit-enumerated</Type>
      <BytePosition>3</BytePosition>
      <Label>Status group 2</Label>
      <Name>device_specific_status_2</Name>
      <AlertList>
        <Alert>
          <Value>128</Value>
          <AlarmString>Unintended Valve Movement</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>64</Value>
          <AlarmString>Valve Open Stuck</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>32</Value>
          <AlarmString>Valve Close Stuck</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>16</Value>
          <AlarmString>Valve Intermediate Stuck</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>8</Value>
          <AlarmString>Supply Pressure Out of Limits</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>4</Value>
          <AlarmString>Supply Pressure Drop</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>2</Value>
          <AlarmString>Too Large Housing Pressure</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>1</Value>
          <AlarmString>Temperature Out of Limits</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
      </AlertList>
    </Variable>
    <Variable>
      <Size>1</Size>
      <Type>bit-enumerated</Type>
      <BytePosition>4</BytePosition>
      <Label>Status group 3</Label>
      <Name>device_specific_status_3</Name>
      <AlertList>
        <Alert>
          <Value>128</Value>
          <AlarmString>Spool Valve Stuck</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>64</Value>
          <AlarmString>Pneumatics Problem</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>32</Value>
          <AlarmString>PST Pressure Drop</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>16</Value>
          <AlarmString>PST Overshoot</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>8</Value>
          <AlarmString>Valve Opening Time High Limit Exceeded</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>4</Value>
          <AlarmString>Valve Closing Time High Limit Exceeded</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>2</Value>
          <AlarmString>Loop Current Below Low Limit</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>1</Value>
          <AlarmString>Free</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
      </AlertList>
    </Variable>
    <Variable>
      <Size>1</Size>
      <Type>bit-enumerated</Type>
      <BytePosition>5</BytePosition>
      <Label>Status group 4</Label>
      <Name>device_specific_status_4</Name>
      <AlertList>
        <Alert>
          <Value>128</Value>
          <AlarmString>Valve Full Strokes Limit Exceeded</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>64</Value>
          <AlarmString>Actuator Full Strokes Limit Exceeded</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>32</Value>
          <AlarmString>PST Counter Limit Exceeded</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>16</Value>
          <AlarmString>Total Operation Time Limit Exceeded</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>8</Value>
          <AlarmString>Free</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>4</Value>
          <AlarmString>Free</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>2</Value>
          <AlarmString>Free</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>1</Value>
          <AlarmString>Free</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
      </AlertList>
    </Variable>
    <Variable>
      <Size>1</Size>
      <Type>bit-enumerated</Type>
      <BytePosition>6</BytePosition>
      <Label>Status group 5</Label>
      <Name>device_specific_status_5</Name>
      <AlertList>
        <Alert>
          <Value>128</Value>
          <AlarmString>Temperature Trend Low Limit</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>64</Value>
          <AlarmString>Temperature Trend High Limit</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>32</Value>
          <AlarmString>Supply Pressure Trend Low Limit</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>16</Value>
          <AlarmString>Supply Pressure Trend High Limit</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>8</Value>
          <AlarmString>PST Breakaway Pressure Low Limit</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>4</Value>
          <AlarmString>PST Breakaway Pressure High Limit</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>2</Value>
          <AlarmString>PST Load Factor Low Limit</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>1</Value>
          <AlarmString>PST Load Factor High Limit</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
      </AlertList>
    </Variable>
    <Variable>
      <Size>1</Size>
      <Type>bit-enumerated</Type>
      <BytePosition>7</BytePosition>
      <Label>Ext dev status</Label>
      <Name>extended_fld_device_status</Name>
      <AlertList>
        <Alert>
          <Value>1</Value>
          <AlarmString>Maintenance required</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>2</Value>
          <AlarmString>Device variable alert</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>4</Value>
          <AlarmString>Critical Power Failure</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
      </AlertList>
    </Variable>
    <Variable>
      <Size>1</Size>
      <Type>bit-enumerated</Type>
      <BytePosition>11</BytePosition>
      <Label>AO saturated</Label>
      <Name>analog_channel_saturated1</Name>
      <AlertList>
        <Alert>
          <Value>1</Value>
          <AlarmString>Secondary Analog Channel Saturated</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>2</Value>
          <AlarmString>Tertiary Analog Channel Saturated</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>4</Value>
          <AlarmString>Quaternary Analog Channel Saturated</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>8</Value>
          <AlarmString>Quinary Analog Channel Saturated</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
      </AlertList>
    </Variable>
    <Variable>
      <Size>1</Size>
      <Type>bit-enumerated</Type>
      <BytePosition>14</BytePosition>
      <Label>AO fixed</Label>
      <Name>analog_channel_fixed1</Name>
      <AlertList>
        <Alert>
          <Value>1</Value>
          <AlarmString>Secondary Analog Channel Fixed</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>2</Value>
          <AlarmString>Tertiary Analog Channel Fixed</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>4</Value>
          <AlarmString>Quaternary Analog Channel Fixed</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>8</Value>
          <AlarmString>Quinary Analog Channel Fixed</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
      </AlertList>
    </Variable>
    <Variable>
      <Size>1</Size>
      <Type>bit-enumerated</Type>
      <BytePosition>15</BytePosition>
      <Label>Status group 14</Label>
      <Name>device_specific_status_14</Name>
      <AlertList>
        <Alert>
          <Value>128</Value>
          <AlarmString>Pressure Sensor 1 Failure</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>64</Value>
          <AlarmString>Pressure Sensor 2 Failure</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>32</Value>
          <AlarmString>Supply Pressure Sensor Failure</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>16</Value>
          <AlarmString>Temperature Sensor Failure</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>8</Value>
          <AlarmString>Position Sensor Out of Range</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>4</Value>
          <AlarmString>Position Sensor Failure</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>2</Value>
          <AlarmString>Input Signal Sensor failure</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>1</Value>
          <AlarmString>Free</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
      </AlertList>
    </Variable>
    <Variable>
      <Size>1</Size>
      <Type>bit-enumerated</Type>
      <BytePosition>16</BytePosition>
      <Label>Status group 15</Label>
      <Name>device_specific_status_15</Name>
      <AlertList>
        <Alert>
          <Value>128</Value>
          <AlarmString>PST Failed</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>64</Value>
          <AlarmString>Emergency Trip Test Failed</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>32</Value>
          <AlarmString>Pneumatics Test Failed</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>16</Value>
          <AlarmString>Safety Electronics Test Failed</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>8</Value>
          <AlarmString>Ready to Reset</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>4</Value>
          <AlarmString>Safety Position Requested</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>2</Value>
          <AlarmString>LCP Communication Failure</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
        <Alert>
          <Value>1</Value>
          <AlarmString>Free</AlarmString>
          <Severity>ALERT_ABNORM_ID</Severity>
          <ExtendedHelpText>
          </ExtendedHelpText>
          <DDHelpText>
          </DDHelpText>
        </Alert>
      </AlertList>
    </Variable>
  </VariableList>
</AlertsRoot>